Best Practices

1. Draw picture of the intended design
   1. Clearly label inputs, output, and bus widths
2. Use clear variable names
3. Comment components as you would in a drawing
4. Design and test incrementally
5. Create concrete test benches
6. Agree on style convention
7. Compile with vcom -work work \*.vhd